{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["初期画面","計算"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"初期画面","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[[35,1,35,3]]}
[null,"　 コイル設計プログラム　PCOEXL"]
[null,null,"品種名","TEST170125"]
[]
[null,null,"参考データ","無し"]
[null,null,"コイル形状","ダブルショート",null,null,21.709945678710937,null,null,0]
[null,null,"分割数",1,null,null,6534.69384765625,null,null,0]
[null,null,"封体内径",8,"mm",null,435.2593994140625,null,null,0]
[null,null,"設計電圧",100,"V",null,23.765354156494141,null,null,9.2989873886108398]
[null,null,"設計電力",300,"W",null,8.8709205389022827E-2,null,null,16.067276000976562]
[null,null,"設計色温度",2800,"K",null,875.8922119140625,null,null,1.1255598068237305]
[null,null,"封入ガス","アルゴン",null,null,882.727783203125,null,null,32.330886840820313]
[null,null,"封入圧",2,"kg/c㎡",null,285.71762084960937,null,null,0.59039568901062012]
[null,null,"ＣＬ1 ",20,"mm",null,0]
[null,null,"ＣＬ2 ",30,"mm",null,0]
[null,null,"巻付ｻﾎﾟｰﾀ数",0,null,null,398.13839721679687]
[null,null,"巻付け数",0,null,null,0]
[null,null,"ｺｲﾙﾘｰﾄﾞ部",0,"mm",null,6.7636728286743164]
[null,null,"ﾘ-ﾄﾞ単線部",30,"mm",null,0]
[null,null,"ｻﾌﾞｺｲﾙ長さ",20,"mm",null,1.0149796009063721]
[null,null,"ＭＤ1",0.6,"mm"]
[null,null,"ＭＤ2",2,"mm"]
[null,null,"効率","--- ","lm/W"]
[null,null,"寿命","--- ","h"]
[null,null,"ＭＧ","--- ","mg/200mm"]
[null,null,"ＵＣＬ","--- ","mm"]
[]
[]
[]
[]
[null,null,null,null,null,"V1.05"]
[]
[]
[]
[]
[]
[null,"入力選択候補"]
[null,"有り","シングルロング","チッ素"]
[null,"無し","シングルショート","アルゴン"]
[null,null,"ダブルロング","Ｋｒ"]
[null,null,"ダブルショート","Ｘｅ"]
[null,null,"C-13"]
[null,null,"C-13D"]
[null,null,"CC-13"]

{"sheet":"計算","index":1,"n_rows":40,"n_cols":10,"rows_kept":40,"cut":false,"hidden":true,"merged":[]}
[]
[null,null,"品種名",{"$f":"初期画面!D2","v":"TEST170125"},null,null,null,null,{"$f":"NOW()","v":"2017-01-25T10:02:10.670"}]
[]
[null,null,"参考データ","無し"]
[null,null,"コイル形状","ダブルショート",null,"効率",14.903839111328125,null,"保温係数修正",1]
[null,null,"分割数",1,null,"光束",4471.15185546875,null,"未確定損失長",0]
[null,null,"封体内径",8,null,"寿命",3728.072509765625,null,"光損失率",0]
[null,null,"設計電圧",100,null,"ＭＧ",61.359291076660156,null,"サポ―タ損失長",0]
[null,null,"設計電力",300,null,"d",0.14253997802734375,null,"リ―ド実効損失長",16.270000457763672]
[null,null,"設計色温度",2800,null,"ＵＣＬ",598.54779052734375,null,"放射保温係数",1.0358122587203979]
[null,null,"封入ガス","アルゴン",null,"ＵＣＬeff",615.0877685546875,null,"ガス電力損失",51.849075317382813]
[null,null,"封入圧",2,null,"ＰＰ1",54.368640899658203,null,"伝導電力損失",0.947532057762146]
[null,null,"ＣＬ1 ",20,null,"ＰＰ2",78005032]
[null,null,"ＣＬ2 ",30,null,"ＰＰin",1E-3]
[null,null,"巻付ｻﾎﾟｰﾀ数",0,null,"ＴＴ1",256.23504638671875]
[null,null,"巻付け数",0,null,"ＴＴ2",0]
[null,null,"ｺｲﾙﾘｰﾄﾞ部",0,null,"ＭＤ1/ｄ",4.2093453407287598]
[null,null,"ﾘ-ﾄﾞ単線部",30,null,"MD2/MD1",3.3333332538604736]
[null,null,"ｻﾌﾞｺｲﾙ長さ",20,null,"コイル外径",3.7701599597930908]
[null,null,"ＭＤ1",0.6]
[null,null,"ＭＤ2",2,null,"青字の項目を修正してください。"]
[]
[]
[null,null,"公称電圧","D26",null,null,null,null,"タングステンメ―カ―指定","Ｊ25"]
[null,null,"公称電力","D27",null,null,null,null,"ｺｲﾙﾒｰｶによる一次熱処理温度","J26"]
[null,null,"追加記号","D28",null,null,null,null,"ｺｲﾙﾒｰｶによる一次熱処理時間","J27"]
[null,null,"定格寿命","D29",null,null,null,null,"ｺｲﾙﾒｰｶによる二次熱処理温度","J28"]
[null,null,"定格光束","D30",null,null,null,null,"ｺｲﾙﾒｰｶによる二次熱処理時間","J29"]
[null,null,"サポータ外径","D31",null,null,null,null,"社内での熱処理温度","J30"]
[null,null,"サポータＭＧ","D32",null,null,null,null,"社内での熱処理時間","J31"]
[null,null,"参考した設計","D33"]
[]
[]
[]
[]
[null,null,null,"ガスリスト"]
[null,null,null,{"$f":"初期画面!D37","v":"チッ素"}]
[null,null,null,{"$f":"初期画面!D38","v":"アルゴン"}]
[null,null,null,{"$f":"初期画面!D39","v":"Ｋｒ"}]
[null,null,null,{"$f":"初期画面!D40","v":"Ｘｅ"}]